# Constant Field Values

## Contents

- edu.sc.*

## edu.sc.*

- edu.sc.seis.TauP.Arrival
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final double` | `DtoR` | `0.017453292519943295`
  `protected static final double` | `RtoD` | `57.29577951308232`
  `protected static final double` | `TWOPI` | `6.283185307179586`

- edu.sc.seis.TauP.PolarPlot
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final short` | `FULL` | `0`
  `public static final short` | `HALF` | `1`
  `public static final short` | `QUARTER` | `2`

- edu.sc.seis.TauP.SeismicPhase
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DIFFRACT` | `5`
  `public static final int` | `END` | `6`
  `public static final int` | `END_DOWN` | `7`
  `public static final boolean` | `PWAVE` | `true`
  `public static final int` | `REFLECT_TOPSIDE` | `2`
  `public static final int` | `REFLECT_TOPSIDE_CRITICAL` | `9`
  `public static final int` | `REFLECT_UNDERSIDE` | `1`
  `public static final int` | `REFLECT_UNDERSIDE_CRITICAL` | `8`
  `public static final boolean` | `SWAVE` | `false`
  `public static final int` | `TRANSDOWN` | `4`
  `public static final int` | `TRANSUP` | `3`
  `public static final int` | `TURN` | `0`

- edu.sc.seis.TauP.Sfun
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final double` | `EPSILON_LARGE` | `2.2204460492503E-16`
  `public static final double` | `EPSILON_SMALL` | `1.1102230246252E-16`

- edu.sc.seis.TauP.SlownessModel
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final double` | `DEFAULT_SLOWNESS_TOLERANCE` | `1.0E-16`
  `public static final boolean` | `PWAVE` | `true`
  `public static final boolean` | `SWAVE` | `false`

- edu.sc.seis.TauP.SphericalCoords
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `protected static final double` | `dtor` | `0.017453292519943295`
  `protected static final double` | `rtod` | `57.29577951308232`

- edu.sc.seis.TauP.TauP_SetSac
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `A_HEADER` | `10`

- edu.sc.seis.TauP.TauP_SlownessPlot
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `DEFAULT_OUTFILE` | `"taup_slownessmodel"`

- edu.sc.seis.TauP.TauP_Table
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `GENERIC` | `0`
  `public static final int` | `LOCSAT` | `1`

- edu.sc.seis.TauP.TauP_Tool
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `GMT` | `"gmt"`
  `public static final java.lang.String` | `JSON` | `"json"`
  `public static final java.lang.String` | `SVG` | `"svg"`
  `public static final java.lang.String` | `TEXT` | `"text"`

- edu.sc.seis.TauP.TauP_VelocityPlot
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `DEFAULT_OUTFILE` | `"taup_velocitymodel"`

- edu.sc.seis.TauP.VelocityModel
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final double` | `DEFAULT_CMB` | `2889.0`
  `public static final double` | `DEFAULT_IOCB` | `5153.9`
  `public static final double` | `DEFAULT_MOHO` | `35.0`